Alcohol breathalyzer instruction sheet

1. Plug breathalyzer into power source through two inputs provided next to sensor.
2. Wait for first green ‘ready’ light to turn on, approx. 100 seconds
3. Blow down tube to get reading.
4. Wait for 5 seconds.
5. Press the reset button.
6. Blow again.

All LEDs may light up instantaneously upon contact of the metal box, simply reset the breathalyzer and run again.

If deconstruction of breathalyzer is required please follow steps outlined below:

1. Undo screws on side.
2. Lift lid slightly, careful not to pull wires out of pins.
3. Find nut holding vero-board to the container.
4. Unscrew and lift.